What is cooking gas  
{  
Cooking gas is Liquefied Petroleum Gas, LPG in short. LPG, as the name implies, is gas in liquid form under pressure. It is filled under pressure in cylinders, stored and then transported to your house.  
}

ho do i book a gas online  
{

Connections are now available on demand in most of the parts of the country. All you need to do is approach the nearest GREENGAS Distributor catering to your area with a proof of identity and proof of your residence address. In case there is a waiting list for new connection at any place, the distributor will register your name for a new connection and give you a waiting list number. Thereafter, he will send you an intimation letter as soon as your turn matures.  
}

what are the parts of your gas installation

{

|  |
| --- |
| A cylinder with a self-closing valve. |
| **»** | A pressure regulator, which is connected to the outlet of the valve. |
| **»** | A gas stove or a cooking range (appliance). |
| **»** | Rubber tube connecting the regulator to the appliance. |

}

how do i take care of your stove  
{

|  |
| --- |
| Harsh cleaners can damage the finish. Don't use abrasive powders, highly acidic or alkaline cleansers. |
| **»** | Wait for surfaces to cool. If the stove is hot and you try to clean it with a wet cloth, the surface finish may crack. |
| **»** | Some foodstuffs can damage the finish. Vinegar, sour milk, citrus fruits juices, tamarind decoctions |
| **»** | can all damage the finish. If some such liquid spills on the stove, wipe it off with a dry cloth, wait for the stove to cool, clean with warm soap water and dry. |
| **»** | Ordinary stains can be cleaned easily. Some baking soda on a damp cloth does the trick. A mild cleanser may be used for stubborn stains. |
| **»** | A chrome finish can be cleaned with a damp cloth. Or any good chrome cleanser. |
| **»** | Clean the burner head and mixing tube the right way. Immerse the mixing tube assembly and the burner head completely in a boiling solution of washing soda. Keep it for 20 minutes. Rinse thoroughly internally and externally. Dry completely to prevent corrosion. |
| **»** | The burner holes should be cleaned with a soft wire. The mixing tube can be cleaned with a stiff bottlebrush. |
| **»** | Pan supports can be cleaned the same way. |

}

things to be done when cyl are to be changed  
{

|  |
| --- |
| Put out all fires in the kitchen. This includes diyas, agarbatties, cigarettes and all naked flames; otherwise any leakage of gas could result in fire. |
| **»** | Switch off all electrical appliances. |
| **»** | Shut the taps on the stove. |
| **»** | Have the rubber tube and all the connections checked for leakage with soap solution. |
| **»** | Insist that your deliveryman checks cylinder valve and O-ring for any leakage. |

}

basic rules of safety

{

|  |
| --- |
| Always remember to shut the value when the stove is not in use, especially at night.Don't tamper with your cylinder or allied equipment. |
| **»** | Make sure all parts of the installation are in good condition. If you find anything wrong with any part, contact your distributor and ask for a mechanic. |
| **»** | It is safer to wear cotton clothing while working in the kitchen.Do not use dupatta to handle utensils, preferably use an apron. |
| **»** | Keep children away from the installation while you're cooking. |
| **»** | Use dry pot holders. |
| **»** | Never leave the hotplate on and unattended. The burners could extinguish by overflow of cooking material or even draught of air) allowing gas to leak. The accumulated gas could get ignited by the second burner in operation (or other sources) resulting in fire. |
| **»** | Turn pan handles to the side away from the flame. Keep plastic items away from the stoves. |
| **»** | 50% of cooking gas-related accidents occur because of leakages from the rubber tube. |
| **»** | Get your tube changed, whenever it is damaged. And as a rule, replace the rubber tube every two years. |
| **»** | Keep the safety cap on over unused cylinders. |

}

what do you do when u smel gas

{

|  |
| --- |
| urn the pressure regulator knob to the OFF position. |
| **»** | Put out all fires in the kitchen (including agarbatti and pooja lamp). |
| **»** | Open all doors and windows for ventilation. |
| **»** | Do not strike a match and do not operate any electric switches (including main switch). |
| **»** | Electrical switches and dry cell torches generate spark while switching on or off. |
| **»** | Get in touch with you distributor or get in touch with your Emergency Service Cell managed by the Oil Companies after office hours and on Sundays and holidays. |

}